B5 Journal

22 March 15

Hillshaded and now going to add algae data.

Finished Matlab. No big issues here. Except that there are very few points throughout the years for this stream.

31 march 15

Redoing the 9394 problem. Working on 0203 when I noticed that there were 2 points almost exactly 1 m off of normal. I am assuming it was another rod mistake. Fixed 0203. Looks much cleaner now. Could have been 0.5 m rise during the flood!

9394 is all over the place, but could have been rocks moved etc.

Or wait, when was the gage built? Nope not gage. Lidar was taken a couple days prior.

7 apr 15

Started up on AFDM with Bohner stream. Why was 1011 and 0203 so big? I forgot and why they hell didn’t I write it down. I wrote 0203 down but that was it.

May need to make a patch that is 9X9 instead of 3X3 for this stream.